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Sampling Report – Products according to EN 14041 / 14342 / 15102 (Order No.      )

	Testing laboratory:
	TFI Aachen GmbH

	
	

	Sampler:
(Organisation and name of person) 
	     

	
	

	Manufacturer / Contractor:
	     

	
	

	Sampling site (factory):
	     



	Product name:
	     
	
	Article number:
	     

	
	
	
	
	

	Group/product range:

	[bookmark: Kontrollkästchen31]|_| CE: 1658-CPR-     
[bookmark: Kontrollkästchen32]|_| DIBt:      
|_| TÜV-Interior: 70 710      
	
	Sample type:
	[bookmark: Kontrollkästchen27]|_| textile floor covering
[bookmark: Kontrollkästchen28]|_| resilient floor covering
[bookmark: Kontrollkästchen29]|_| laminate
[bookmark: Kontrollkästchen39]|_| wood flooring
[bookmark: Kontrollkästchen30]|_| surface for sports areas
|_|      

	
	
	
	
	

	Batch no.:
	     
	
	Production date of batch:
	     



	Sampling date and time:
	      /      

	
	
	
	
	

	Sample taken from:
	|_| production
|_| stock
|_| retain sample
	
	Storage mode:
	|_| exposed
|_| packed 

	
	
	
	
	

	Storage location:
	     
	
	Packaging material:
	     

	
	
	
	
	

	Size of sample:
	     



	Particular remarks: 
(Possible negative impacts caused by emissions at the sampling site, problems, questions etc.)
	|_| taken as retain sample according to MVV TB instructions
[bookmark: Kontrollkästchen33]|_| gas driven forklift	|_| monitoring testing based on approval principles
     

	

	Planned tests:
[bookmark: Kontrollkästchen18][bookmark: Kontrollkästchen25][bookmark: Kontrollkästchen26]|_| construction features			|_| formaldehyde				|_| PCP
[bookmark: Kontrollkästchen14][bookmark: Kontrollkästchen15][bookmark: Kontrollkästchen16][bookmark: Kontrollkästchen19]|_| determination of fire class (RP)		|_| RP red. number of samples		|_| Small Burner Test
|_| emission testing (Initial type test)	|_| emission testing (Monitoring)
|_| TÜV-Interior Emission Monitoring	|_| Standard	|_| Premium	Allocation criteria V     
|_| TÜV-Interior Quality Monitoring

	Fire class:
	     
	[bookmark: Kontrollkästchen37]|_| unglued	|_| glued with:      



	[bookmark: Kontrollkästchen34]|_| 
	technical datasheet will be submitted to TFI within 3 days
	[bookmark: Kontrollkästchen35]|_|
	technical datasheet is attached

	Hereby the signatories confirm the correctness of the above information. The sample was hand selected and packed in accordance with the sampling instructions.

	
	Signature of the sampler (in case of third party sampling)
	
	Signature of the company
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TFI Aachen GmbH Charlottenburger Allee 41
52068 Aachen ∙ Germany
Tel: +49.241.9679 00
www.tfi-aachen.de

Notified Body
 No. 1658
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